
Activity:

Soil Moisture #2



Description:

Build a program that will read the soil moisture value and display the value onto the screen using a loop. The soil moisture value will be read with a given soil moisture sensor.

Vocabulary and Concepts:

**Soil Moisture Sensor**: sensor that estimate volumetric water content

**Iteration (Loop):** A repetitive action or command typically created with programming loops. Loop action of doing something repeatedly.

Flowchart:

A flowchart is a way of representing the step-by-step process (algorithm) of your program. For this program, the flowchart is:

This program contains a while loop that is always true meaning the program will never end. In that case, the flow chart will not consist of an end circle.

Diagram

Description automatically generated with medium confidence

Build the Circuit

**Materials Required:**

* gator:soil - micro:bit Accessory Board
* gator:bit v2.0 – micro:bit carrier board
* Three Crocodile Clips

|  |  |  |
| --- | --- | --- |
| Contact from gator:soil | Connection to gator:bit v2.0 | Connector |
| PWR (power) | P1 | Crocodile Clip |
| SIG (signal) | P0 | Crocodile Clip |
| GND (ground) | GND (ground) | Crocodile Clip |

**Hardware Hookup:**

A picture containing electronics

Description automatically generated

A picture containing text, electronics, circuit

Description automatically generated

**Instructions:**

1. Place gator:soil sensor in soil



Let’s Start Programming!

Step 1: Getting Started

This program will consist of the same process with the Soil\_Moisture1 program. First, we will use the Gator Soil extension for this program. The extension can be used by clicking the “extensions” tab and typing “Gator Soil” into the extensions search bar. Next, the gator soil extension should pop up. Click the extension and the gator soil tab should now appear along with the other tabs. Click the gator soil tab to grab the get moisture block. Set pin P0 in moisture using power pin P1. Finally, the difference is this program is that a loop is used in this program. The loop that will be used is the while true loop which can be found in the loops tab and place all other blocks.

**Extensions:**

* GatorSoil

A picture containing table

Description automatically generated

Step 2: Selection Changes

Changes may consist of changing to any pin number, but P0 and P1 are good choices for now.

The ADCValue may also be changed to moisture. The ADC value is the moisture value divided by 100.

Step 3: Test your Program using the Emulator

Since it is a loop, test your program by pressing start on the emulator and changing the value of the pin 0 by clicking on pin 0 on the microbit and dragging up and down along the pin.

Graphical user interface

Description automatically generated with low confidence




Step 4: Connect to your micro:bit

Step 5: Download the Program

Step 6: Running the Program on the micro:bit

Congratulations!

You have created your Soil Sensor program!!

References

Online Moisture Sensor tutorial: <https://youtu.be/S8NppVT_paw>

SparkFun gator:soil Hookup Guide: <https://learn.sparkfun.com/tutorials/sparkfun-gatorsoil-hookup-guide?_ga=2.146091443.620133083.1655840734-1398352755.1654058977>

Flowchart tool: <https://www.draw.io/>